# Implement Network Configuration - PVDU

PhysicalFunction

In-Flight Entertainment System > In-Flight Entertainment System > Physical Architecture > Physical Functions > Root Physical Function > IFE System > Distribute data > Implement Network Configuration - PVDU

The network distribution is an essential part of the IFE system. This function receives network configurations (IP address, maximum bandwidth, etc.) from the central network management and implements it on the PVDU.

## Incoming Functional Exchanges

Exchange | Source | Description | Allocated Exchange Items
--- | --- | --- | ---
Network Configuration | Reconfigure Network |  |
Network Configuration | Define Initial Network Configuration |  |

## Diagrams displaying "Implement Network Configuration - PVDU"

- RPL - Instantiations of Unit Network Adapter
- [PAB] [BUILD] Template
- [PFBD] All Physical Functions
- [PAB] Focus on Network Transport
- [PAB] Focus on Network Setup, Configuration and Tests