# Capture Aircraft Notifications and Parameters

LogicalFunction

In-Flight Entertainment System > In-Flight Entertainment System > Logical Architecture > Logical Functions > Root Logical Function > IFE System > Provide Aircraft Interface > Capture Aircraft Notifications and Parameters

This function is concentrating the reception of the messages / notifications sent by the aircraft. The implementation of this function is likely to be specific to each aircraft model: The format of the incoming messages is defined by the aircraft manufacturer.

## Incoming Functional Exchanges

Exchange | Source | Description | Allocated Exchange Items
--- | --- | --- | ---
Power Consumption Cap | Provide Electrical Power |  |
Decompression Notificaton | Send Decompression Notification |  |

## Outgoing Functional Exchanges

Exchange | Target | Description | Allocated Exchange Items
--- | --- | --- | ---
Decompression Notification | Determine Operating Profiles |  |
Power Consumption Profile | Determine Operating Profiles |  |

## Realized Elements

- Determine Operating Profiles

## Realizing Elements

- Capture Aircraft Notifications and Parameters

## Diagrams displaying "Capture Aircraft Notifications and Parameters"

- [LAB] [BUILD] All Components, Functions, CEs, FEs
- [LAB] [BUILD] Template
- [FS] Handle Cabin Decompression Event
- [LFBD] All Functions
- [LDFB] [CTX] Provide Aircraft Interface
- [LAB][CTX] Broadcast Audio Announcement FC