# Retrieve Imposed Video Data

PhysicalFunction

In-Flight Entertainment System > In-Flight Entertainment System > Physical Architecture > Physical Functions > Root Physical Function > IFE System > Run Services > Run Cabin Intercommunication Service > Retrieve Imposed Video Data

This function consists in receiving media information requests (list of imposed videos, available languages, etc.) and returning the data corresponding to these requests. This data is retrieved from the digital media storage unit.

## Incoming Functional Exchanges

Exchange | Source | Description | Allocated Exchange Items
--- | --- | --- | ---
Imposed Video Selection Command | Capture Imposed Video Selections |  |
Imposed Video Data | Store Digital Media |  |
Imposed Video List | Store Digital Media |  |

## Outgoing Functional Exchanges

Exchange | Target | Description | Allocated Exchange Items
--- | --- | --- | ---
Available Imposed Video List | Display Imposed Video Data |  |
Media Content Request | Store Digital Media |  |

## Realized Elements

- Retrieve Imposed Video Data

## Diagrams displaying "Retrieve Imposed Video Data"

- [PAB] [BUILD] All PCs, PFs, FEs
- [PAB] [BUILD] Template
- [PFBD] All Physical Functions
- [PDFB] [CTX] Run Cabin Intercommunication Service