# Set Passenger Service Authorization

PhysicalFunction

In-Flight Entertainment System > In-Flight Entertainment System > Physical Architecture > Physical Functions > Root Physical Function > Perform Maintenance, Configuration and Test Operations > Set Passenger Service Authorization

The airline company may have specific business strategies: According to the class they are travelling in, passengers may benefit from different IFE services. This function consists in uploading a profile that describes the authorization schemes.

## Outgoing Functional Exchanges

Exchange | Target | Description | Allocated Exchange Items
--- | --- | --- | ---
Passenger Service Authorization Profile | Determine Passenger Service Availability |  |

## Realized Elements

- Set Passenger Service Authorization

## Diagrams displaying "Set Passenger Service Authorization"

- [PAB] [BUILD] All PCs, PFs, FEs
- [PAB] [BUILD] Template
- [PFBD] All Physical Functions
- [PDFB] [CTX] Manage Passenger Services Lifecycle