# Store interrupted VOD Movie Status

PhysicalFunction

In-Flight Entertainment System > In-Flight Entertainment System > Physical Architecture > Physical Functions > Root Physical Function > IFE System > Run Services > Run Video-On-Demand Service > Store interrupted VOD Movie Status

This function is in charge of storing the current status of the interrupted / deactivated VOD service (in particular, the current selection movie and the current position in this movie).

## Incoming Functional Exchanges

Exchange | Source | Description | Allocated Exchange Items
--- | --- | --- | ---
VOD Movie Interruption Command | Handle VOD Service Activation and Interruption |  |

## Outgoing Functional Exchanges

Exchange | Target | Description | Allocated Exchange Items
--- | --- | --- | ---
VOD Movie Status | Handle VOD Service Activation and Interruption |  |

## Realized Elements

- Store Interrupted VOD Movie Status

## Diagrams displaying "Store interrupted VOD Movie Status"

- [PAB] [BUILD] All PCs, PFs, FEs
- [PAB] [BUILD] Template
- [PFBD] All Physical Functions
- [PAB] Focus on SVDU Audio Video Playing
- [PDFB] [CTX] Run Video-On-Demand Service