# PTV Video Player

PhysicalComponent

In-Flight Entertainment System > In-Flight Entertainment System > Physical Architecture > IFE System > BEHAVIOURAL PCs > PVDU SW > PVDU Video Player > PTV Video Player

No description.

## Allocated Functions

- Store interrupted VOD Movie Status
- Split Audio Video Streams
- Synchronize Audio Video

## Provided Interfaces

- Interfaces.Streaming Protocol

  - For | Streaming Server
    Through | CP 1

## Incoming Component Exchanges

Exchange | Source | Description | Allocated Functional Exchanges | Allocated Exchange Items
--- | --- | --- | --- | ---
Streaming Protocol | Streaming Server |  | Packetized Audio Video Stream Stream Header |

## Outgoing Component Exchanges

Exchange | Target | Description | Allocated Functional Exchanges | Allocated Exchange Items
--- | --- | --- | --- | ---
Packet Transmission | PVDU Video Decoder |  |  |

## Ports

- CP 1
- CP 2

## Diagrams displaying "PTV Video Player "

- [PAB] [BUILD] All PCs, PFs, FEs
- [PAB] [BUILD] Template
- [PAB] Focus on SVDU Audio Video Playing
- [PAB] Implementation and Behaviour Components
- [PCBD] Behavioural Components
- [PAB] [CTX] Start Playing VOD Movie FC
- [PAB] Focus on Network Transport