# Send Decompression Notification

LogicalFunction

In-Flight Entertainment System > In-Flight Entertainment System > Logical Architecture > Logical Functions > Root Logical Function > Provide Aircraft Information, Commands and Means > Send Decompression Notification

If ever a decompression occurs, a notification is sent to the IFE system (which will automatically swtich to "Halted" mode.

## Outgoing Functional Exchanges

Exchange | Target | Description | Allocated Exchange Items
--- | --- | --- | ---
Decompression Notificaton | Capture Aircraft Notifications and Parameters |  |

## Realized Elements

- Send Decompression Notification

## Realizing Elements

- Send Decompression Notification

## Diagrams displaying "Send Decompression Notification"

- [LAB] [BUILD] All Components, Functions, CEs, FEs
- [LAB] [BUILD] Template
- [LFBD] All Functions