# Define Initial Network Configuration

PhysicalFunction

In-Flight Entertainment System > In-Flight Entertainment System > Physical Architecture > Physical Functions > Root Physical Function > IFE System > Distribute data > Setup Network > Define Initial Network Configuration

The network distribution is an essential part of the IFE system. This function creates the configurations for all connected equipments (IP address, maximum bandwidth, etc.).

## Outgoing Functional Exchanges

Exchange | Target | Description | Allocated Exchange Items
--- | --- | --- | ---
Network Configuration | Implement Network Configuration |  |
Network Configuration | Implement Network Configuration - CMU |  |
Network Configuration | Implement Network Configuration - PVDU |  |

## Diagrams displaying "Define Initial Network Configuration"

- [PAB] [BUILD] Template
- [PFBD] All Physical Functions
- [PAB] Focus on Network Setup, Configuration and Tests