# Interrupt Current Service

PhysicalFunction

In-Flight Entertainment System > In-Flight Entertainment System > Physical Architecture > Physical Functions > Root Physical Function > IFE System > Manage Passenger Services Lifecycle > Interrupt Current Service

This function is responsible for triggering passenger service interruptions as soon as an imposed video is played or an audio announcement is performed. When a VOD movie is running, this means for example that the movie as to be automatically paused and the current position stored.

## Incoming Functional Exchanges

Exchange | Source | Description | Allocated Exchange Items
--- | --- | --- | ---
Service Interruption Command | Process Imposed Video Controls |  |
Service Interruption Command | Process Audio Announcement |  |

## Outgoing Functional Exchanges

Exchange | Target | Description | Allocated Exchange Items
--- | --- | --- | ---
Service Interruption Command | Handle VOD Service Activation and Interruption |  |
Audio Interruption Notification | Display Audio Interruption Screen on Seat TV |  |

## Realized Elements

- Interrupt Current Service

## Diagrams displaying "Interrupt Current Service"

- [PAB] [BUILD] All PCs, PFs, FEs
- [PAB] [BUILD] Template
- [PFBD] All Physical Functions
- [PDFB] [CTX] Manage Passenger Services Lifecycle