# Receive Imposed Video Playing Status

LogicalFunction

In-Flight Entertainment System > In-Flight Entertainment System > Logical Architecture > Logical Functions > Root Logical Function > IFE System > Manage Audio and Video Diffusion > Display Video and Play Audio > Receive Imposed Video Playing Status

This function collects the status of the currently running imposed movie (ETA, etc.). This status is then transmitted to be displayed on the Cabin Management Terminal.

## Incoming Functional Exchanges

Exchange | Source | Description | Allocated Exchange Items
--- | --- | --- | ---
Pause-Stop Notification | Prepare Broadcasts |  |
Imposed Video Playing Status | Prepare Broadcasts |  |

## Outgoing Functional Exchanges

Exchange | Target | Description | Allocated Exchange Items
--- | --- | --- | ---
Imposed Video Status | Display Imposed Video Playing Status on Cabin Terminal |  |

## Realized Elements

- Broadcast Audio Video Streams

## Realizing Elements

- Receive Imposed Video Playing Status

## Diagrams displaying "Receive Imposed Video Playing Status"

- [LAB] [BUILD] All Components, Functions, CEs, FEs
- [LAB] [BUILD] Template
- [LDFB] [CTX] Display Video and Play Audio
- [LFBD] All Functions
- [LAB][CTX] Watch Imposed Video on Cabin Screen FC