# Play Video Stream on Cabin Screen

PhysicalFunction

In-Flight Entertainment System > In-Flight Entertainment System > Physical Architecture > Physical Functions > Root Physical Function > IFE System > Manage Audio Video Diffusion > Display Video and Play Audio > Play Video Stream on Cabin Screen

This function receives video packets and restitutes the corresponding video through the cabin screens. The audio track associated to the video is forwarded to the aircraft through another function.

## Incoming Internal Functional Exchanges

Exchange | Source | Target | Description | Allocated Exchange Items
--- | --- | --- | --- | ---
Packetized Video Stream | Send Audio Video Packet | Receive and Bufferize Video Packet |  |
Pause-Stop Notification | Prepare Broadcasts | Decode Video Packet |  |

## Outgoing Internal Functional Exchanges

Exchange | Source | Target | Description | Allocated Exchange Items
--- | --- | --- | --- | ---
Played Video | Decode Video Packet | Display Video on Cabin Screen |  |

## Realized Elements

- Play Video Stream on Cabin Screen

## Owned diagrams

[PDFB] [CTX] Play Video Stream on Cabin Screen

## Diagrams displaying "Play Video Stream on Cabin Screen"

- [PDFB] [CTX] Display Video and Play Audio
- [PFBD] All Physical Functions