# Capture Passenger Service Selection

PhysicalFunction

In-Flight Entertainment System > In-Flight Entertainment System > Physical Architecture > Physical Functions > Root Physical Function > IFE System > Manage Passenger Services Lifecycle > Capture Passenger Service Selection

This function handles the general interactions with the passenger. The Seat TV displays interaction widgets (typically buttons and slide bars). This typically airline-specifc, because user interface typically is. This function is responsible for capturing the selections of services and forwarding them to a more generic function (a controler) that will transform the selections into an internal system commands (activation / de-activation).

## Incoming Functional Exchanges

Exchange | Source | Description | Allocated Exchange Items
--- | --- | --- | ---
Passenger Homepage Selection | Select Passenger Service |  |
VOD Service Selection | Select Passenger Service |  |

## Outgoing Functional Exchanges

Exchange | Target | Description | Allocated Exchange Items
--- | --- | --- | ---
Service Deasctivation Command | Store Passenger Service State |  |
VOD Service Activation Command | Start/Resume Service |  |
Passenger Homepage Display Command | Display Homepage on Seat TV |  |

## Realized Elements

- Capture Passenger Service Selection

## Diagrams displaying "Capture Passenger Service Selection"

- [PAB] [BUILD] Template
- [PFBD] All Physical Functions
- [PDFB] [CTX] Manage Passenger Services Lifecycle