# Store Interrupted VOD Movie Status

LogicalFunction

In-Flight Entertainment System > In-Flight Entertainment System > Logical Architecture > Logical Functions > Root Logical Function > IFE System > Run Services > Run Video-On-Demand Service > Store Interrupted VOD Movie Status

This function is in charge of storing the current status of the interrupted / deactivated VOD service (in particular, the current selection movie and the current position in this movie).

## Incoming Functional Exchanges

Exchange | Source | Description | Allocated Exchange Items
--- | --- | --- | ---
VOD Movie Interruption Command | Handle VOD Service Activation and Interruption |  |

## Outgoing Functional Exchanges

Exchange | Target | Description | Allocated Exchange Items
--- | --- | --- | ---
VOD Movie Status | Handle VOD Service Activation and Interruption |  |

## Realized Elements

- Manage Passenger Service Interruptions

## Realizing Elements

- Store interrupted VOD Movie Status

## Diagrams displaying "Store Interrupted VOD Movie Status"

- [FS] Perform Audio Announcement
- [LAB] [BUILD] All Components, Functions, CEs, FEs
- [LAB] [BUILD] Template
- [LDFB] [CTX] Run Video-On-Demand Service
- [LFBD] All Functions
- [ES] Perform Audio Announcement
- [LAB][CTX] Start Playing VOD Movie FC
- [LAB][CTX] Broadcast Audio Announcement FC