# Streaming Server

PhysicalComponent

In-Flight Entertainment System > In-Flight Entertainment System > Physical Architecture > IFE System > BEHAVIOURAL PCs > Aircraft Front Servers > VSU SW > Streaming Server

No description.

## Allocated Functions

- Send Audio Video Packet
- Initiate Audio-Video Stream
- Prepare Broadcasts

## Provided Interfaces

- Interfaces.Media Files

  - For | Media Server
    Through | FIP 1

- Interfaces.VOD Movie Control Command

  - For | PVDU Core Interactions Manager
    Through | FIP 2

## Required Interfaces

- Interfaces.Streaming Protocol

  - From | PTV Video Player
    Through | CP 1

- Interfaces.Media Request

  - From | Media Server
    Through | FOP 5

## Outgoing Component Exchanges

Exchange | Target | Description | Allocated Functional Exchanges | Allocated Exchange Items
--- | --- | --- | --- | ---
Streaming Protocol | PTV Video Player |  | Packetized Audio Video Stream Stream Header |

## Ports

- CP 1
- FOP 5
- FIP 1
- FIP 2

## Realized Elements

- Streaming Server

## Owned diagrams

[CDI] Streaming Server

## Diagrams displaying "Streaming Server"

- [PAB] [BUILD] All PCs, PFs, FEs
- [PAB] [BUILD] Template
- [PAB] Implementation and Behaviour Components
- [PCBD] Behavioural Components
- [PAB] [CTX] Watch Imposed Video on Cabin Screen FC
- [EAB] Configuration Items and Realized Artefacts
- [PAB] [CTX] Start Playing VOD Movie FC
- [PAB] Focus on Network Transport